SATYAPRIYA ROY COLLEGE OF EDUCATION

AA-287, SECTOR-1, SALT LAKE, KOLKATA-700 064

NOTICE

Sealed tenders are invited from bonafide electric contractors for the following works of the college within 7 days from the date of issue of this letter.

1. Earthing

|  |  |  |
| --- | --- | --- |
| SL. NO. | DESCRIPTION | QUANTITY |
| 1 | 600/600 Plate-2Pcs  50x6 Patti-24MTR  25x3 Patti-30MTR | 80 |
| 2 | Charchol | 400 |
| 3 | Salt | 200 |

**Sd/- Principal**

**Satyapriya Roy College of Education**

SATYAPRIYA ROY COLLEGE OF EDUCATION

AA-287, SECTOR-1, SALT LAKE, KOLKATA-700 064

NOTICE

Sealed tenders are invited from bonafide electric contractors for the following works of the college within 7 days from the date of issue of this letter.

2. Main line installation

|  |  |  |
| --- | --- | --- |
| SL. NO. | DESCRIPTION | QUANTITY |
| 1 | Supply & Laying 10MM Coper Nonurmourd Cable | 100 |

**Sd/- Principal**

**Satyapriya Roy College of Education**

SATYAPRIYA ROY COLLEGE OF EDUCATION

AA-287, SECTOR-1, SALT LAKE, KOLKATA-700 064

NOTICE

Sealed tenders are invited from bonafide electric contractors for the following works of the college within 7 days from the date of issue of this letter.

3. Main Switch Fixing & Lift room wiring

|  |  |  |
| --- | --- | --- |
| SL. NO. | DESCRIPTION | QUANTITY |
| 1 | 63A MP 440 V Main Switch | 2 |
| 2 | 32A MP 220 V Main Switch | 1 |
| 3 | Bucket | 4 |
| 4 | 1.5 MM Cable | 2 |
| 5 | Pipe guthka and accessories | 1 |
| 6 | Labour Charge | 1 |

**Sd/- Principal**

**Satyapriya Roy College of Education**

SATYAPRIYA ROY COLLEGE OF EDUCATION

AA-287, SECTOR-1, SALT LAKE, KOLKATA-700 064

NOTICE

Sealed tenders are invited from bonafide electric contractors for the following works of the college within 7 days from the date of issue of this letter.

4. Supply & Fixing Electrical Main Panel Board change

|  |  |  |
| --- | --- | --- |
| SL. NO. | DESCRIPTION | QUANTITY |
| 1 | Supply & Fixing Electric Panel Board | 1 |

**Sd/- Principal**

**Satyapriya Roy College of Education**